### 第四章作业

#### 4-15

The propagation delay

For the sender to seize the channel (sending RTS and CTS),

The transmission delay for the data frames (including overhead)

For the receiver to seize the channel (for sending ACK),

The transmission delay for ACK frame

The effective data rate

#### 4-16

The propagation delay

The minimum time to send a data frame

The minimum frame size